{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["信息点位表","设备清单"],"read":"whole","date_system":"1900"}

{"sheet":"信息点位表","index":0,"n_rows":49,"n_cols":12,"rows_kept":49,"merged":[[0,0,0,11],[1,0,2,0],[1,1,2,2],[1,3,1,5],[1,6,1,7],[1,8,1,11],[3,0,3,11],[4,1,4,2],[4,6,22,6],[4,7,22,7],[4,11,22,11],[5,1,6,1],[7,1,11,1],[12,1,13,1],[12,8,13,8],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,0,23,2],[24,0,24,11],[25,1,25,2],[25,6,46,6],[25,11,46,11],[26,1,27,1],[26,4,27,4],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,41,1],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,0,47,2],[48,0,48,2]]}
["网络信息点位表"]
["楼层","位置",null,"信息点位",null,null,"办公网络设备",null,"监控","监控"]
[{"$nulls":3},"网络","壁挂AP","叫号屏","24口交换机","汇聚交换机","人脸门禁","800万摄像半球","400万电梯摄像机","24口POE交换机"]
["1、一楼信息点位"]
[1,"机房"]
[2,"操作间","操作间"]
[3,null,"值班室"]
[4,"大厅","签到机"]
[5,null,"自助机"]
[6,null,"导诊台"]
[7,null,"直饮水"]
[8,null,"等候区"]
[9,"西药房","3个取药室"]
[10,null,"调剂台"]
[11,"换药室"]
[12,"诊室三"]
[13,"诊室二"]
[14,"诊室一"]
[15,"中药房一","3个取药室"]
[16,"中药房二","2个取药室"]
[17,"消控室"]
[18,"走廊"]
[19,"校内人员入口"]
["1、一楼信息点位小计",null,null,{"$f":"SUM(D5:D23)","v":0},0,0,0,0,0,0,null,{"$f":"SUM(L5:L23)","v":0}]
["2、二楼信息点位"]
[1,"中医特色门诊"]
[2,"针灸康复科","医生急诊台"]
[3,null,"针灸康复科"]
[4,"检验科"]
[5,"诊室七"]
[6,"B超室+心电图室"]
[7,"诊室八"]
[8,"挂号/收费室"]
[9,"中医准备间"]
[10,"西医准备间"]
[11,"注射室"]
[12,"诊室四"]
[13,"诊室五"]
[14,"诊室六"]
[15,"门诊物质存放间"]
[16,"门诊物质存放间走廊区","签到机"]
[17,null,"自助机"]
[18,"男休息室"]
[19,"女休息室"]
[20,"走廊"]
[21,"楼梯间"]
[22,"电梯"]
["2、二楼信息点位小计",null,null,{"$f":"SUM(D26:D47)","v":0},0,0,0,null,{"$f":"SUM(I26:I47)","v":0},0,0,0]
["信息汇总合计",null,null,{"$f":"D48+D24","v":0},0,0,0,0,0,0,0,0]

{"sheet":"设备清单","index":1,"n_rows":45,"n_cols":9,"rows_kept":45,"merged":[[0,0,0,8],[2,0,2,8],[3,8,12,8],[13,0,13,5],[13,6,13,7],[14,0,14,8],[15,8,23,8],[24,0,24,5],[24,6,24,7],[25,0,25,8],[26,8,34,8],[35,0,35,5],[35,6,35,7],[36,0,36,3],[36,4,36,7],[37,0,37,8],[38,0,44,0],[38,1,38,8],[39,1,39,8],[40,1,40,8],[41,1,41,8],[42,1,42,8],[43,1,43,8],[44,1,44,8]]}
["赣州市中医院赣南科技学院综合门诊部信息化项目"]
["序号","项目","品牌","技术指标及性能说明","数量","单位","单价","金额","备注"]
["一、综合布线系统"]
[1,"信息面板",{"$nulls":3},"个",null,null,"1、如有漏项请自行添加项。\n2、排队叫号系统只需要预留信息点位。"]
[2,"底盒",{"$nulls":3},"个"]
[3,"信息模块",{"$nulls":3},"个"]
[4,"六类网线",{"$nulls":3},"箱"]
[5,"2米LC-LC双芯单模光纤跳线",{"$nulls":3},"根"]
[6,"PVC线槽/辅材",null,"￠20-40 PVC线槽，国标阻燃，线槽接口卡、弯头等",null,"米"]
[7,"网络机柜",{"$nulls":3},"个"]
[8,"理线器",{"$nulls":3},"个"]
[9,"辅材",null,"扎带、电工胶布、标签纸、供电电缆等。",null,"批"]
[10,"安装实施费用",null,"项目安装实施费用",null,"项"]
["一、综合布线系统小计：",{"$nulls":5},{"$f":"SUM(H4:H13)","v":0}]
["二、网络设备系统"]
[1,"汇聚交换机",null,"交换机为全网管交换机，支持通过ssh配置和管理；汇聚交换机需配堆叠线缆",null,"台",null,null,"1、如有漏项请自行添加项。\n2、UPS供电时长30分钟以上。\n3、UPS安装含电池连接线、电缆及开关等辅材。"]
[2,"48口接入交换机",null,"交换机为全网管交换机，支持通过ssh配置和管理；汇聚交换机需配堆叠线缆",null,"台"]
[3,"24口POE交换机",null,"交换机为全网管交换机，支持通过ssh配置和管理；汇聚交换机需配堆叠线缆",null,"台"]
[4,"吸顶AP",null,"AP需自带AC功能，可管理其他AP",null,"台"]
[5,"光模块",{"$nulls":3},"块"]
[6,"UPS主机",null,"UPS需提供串口通信模块和协议文档；在线式UPS（5年以上质保）",null,"台"]
[7,"UPS电池组",null,"12V100AH 铅酸免维护蓄电池（5年以上质保）",null,"块"]
[8,"UPS电池柜",{"$nulls":3},"套"]
[9,"安装实施费用",null,"安装实施费用",null,"项"]
["二、网络设备系统小计：",{"$nulls":5},{"$f":"SUM(H16:H24)","v":0}]
["三、安防监控系统"]
[1,"综合安防一体机","大华",null,null,"台",null,null,"1、如有漏项请自行添加项。\n2、监控品牌要求：大华，存储90天。"]
[2,"800万网络摄像机","大华",null,null,"台"]
[3,"400万电梯半球摄像机","大华",null,null,"台"]
[4,"电梯网桥","大华",null,null,"对"]
[5,"8K智能硬盘录像机","大华",null,null,"台"]
[6,"硬盘",null,"16T硬盘",null,"块"]
[7,"43寸显示器",null,"43寸安防显示器",null,"台"]
[8,"辅材",null,"扎带、电工胶布、标签纸、供电电缆等。",null,"批"]
[9,"安装实施费用",null,"项目安装实施费用",null,"项"]
["三、安防监控系统小计",{"$nulls":5},{"$f":"SUM(H27:H35)","v":0}]
["以上设备合计金额（一+二+三）：",{"$nulls":3},{"$f":"G36+G25+G14","v":0}]
[]
["需求","赣南科技学院综合门诊部需求建议"]
[null,"1.叫号系统：所有诊室门口、DR机房门口、检验科门口、B超心电图室门口，预留1组网络和1组强电放置叫号屏。一楼西药房、中药房每个窗口上方，预留1组网络和1组强电放43寸叫号屏。一楼大厅和二楼走廊候诊区墙面，各预留2组网络和2组强电放签到机和叫号屏。"]
[null,"2.监控系统：校外出入口、校内出入口、楼梯间、电梯、大厅、走廊、中药房窗口、西药房窗口、中药房分装中药桌上方，消控室内，均配置安装800万摄像半球，预留网线。消控室配置监控存储及监控主机电脑，监控保存时间90天以上。"]
[null,"3.一楼楼梯间做为弱电信息汇集区域，需要增加一个弱电机柜。"]
[null,"4.DR操作间、所有诊室、检验、B超室、中医特色、针康科、中药房、西药房、挂号收费预留4个网口。注射室、男女休息室预留2个网口。"]
[null,"5.自助机一楼二楼，每台需预留2个网口和1组强电。"]
[null,"6.B超心电图、康复科、中医护理室，吊顶上各预留1组网络，无线AP内网使用。"]